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SPARS -

MAIN MAST

21' 10" overall, round section

Bury below partner = 3'8"

Lower 6'6" constant section 100mm O.D.

Upper taper 15'4" long, 60mm O.D. at tip

Lower half 4mm wall carbon/epoxy layup

Taper wall to 3mm at tip.

Add outside chafing layup at boom and yard contact areas.

MAIN BOOM
Approx. 12'0" overall
2" O.D. with 2mm wall

MAIN YARD
Approx. 14' 4" overall
2" O.D. with 2mm wall

FORE MAST

19'6" overall, round section

Bury below partner = 3'10"

Lower 6'0" constant section, 100mm O.D.

Upper taper 13'6" long, 60mm O.D. at tip.

Lower half 4mm wall carbon/epoxy layup.

Taper wall to 3mm at tip.

Add outside chafing layup at boom and yard contact areas.

FORE BOOM
Approx. 9'7" overall
2" O.D. with 2mm wall

FORE YARD
Approx 11'10" overall
2" O.D. with 2mm wall

Main Sail

1 6'—22"

14

12'-

re—

3"

MacGregor 26
Modified Rig
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