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TR DESIGN - Boat Design By Tad Roberts
PO Box 33 Gabriola Island BC Canada V0R 1X0
email tadrobertsdesign@gmail.com


SPARS -


MAIN MAST
21' 10" overall, round section
Bury below partner = 3'8"
Lower 6'6" constant section 100mm O.D.
Upper taper 15'4" long, 60mm O.D. at tip
Lower half 4mm wall carbon/epoxy layup
Taper wall to 3mm at tip.
Add outside chafing layup at boom and yard contact areas.


MAIN BOOM
Approx. 12'0" overall
2" O.D. with 2mm wall


MAIN YARD
Approx. 14' 4" overall
2" O.D. with 2mm wall


FORE MAST
19'6" overall, round section
Bury below partner = 3'10"
Lower 6'0" constant section, 100mm O.D.
Upper taper 13'6" long, 60mm O.D. at tip.
Lower half 4mm wall carbon/epoxy layup.
Taper wall to 3mm at tip.
Add outside chafing layup at boom and yard contact areas.


FORE BOOM
Approx. 9'7" overall
2" O.D. with 2mm wall


FORE YARD
Approx 11'10" overall
2" O.D. with 2mm wall
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