STORAGE COMMERCIAL DECK BARGE.
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   WATER AREA.                 DECK GUNWALE
                                                                  FUEL AREA.
                         MANHOLE                      VENT 
RAKE KNUCKLE                          45digree point
                  DIESEL AREA                                  ENGINE OIL AREA.
                                  SUFFICIENT PIECES OF TYRE FENDER ALL AROUND
          BILGE KNUCKLE
                                     VERTICAL STANCHION FOR ANCHOR WINCH SUPPORT 
1 X 900 KG ANCHOR C/W A MANUAL ANCHOR WINCH                             

                                                                         Flutter
THE STRUCTURAL LAYOUT OF THE INTERIOR PARTITIONS & BRAZES, FENDER, FLOATER OF A 12M X 60M DECK BARGE.





                             48m
Earth plate

DIAGRAME SHOING THE DIAMENTION FOR EVERY PARTITION.


4m
4m

INTERIOR BRAZING METHODE SHOWING THE VERTICAL ,DIAGONAL, STANCHTIONS AND TRANSVERSE TRUSS.



DIAGRAM SHOWING THE PRODOCT SUPPLY LINES IN VARIOUS SECTIONS.
1. The red manhole covers are for desil.

2. The black manhole covers are for engine oil.

3. The gold manhole covers are for fuel.

4. The fent black manhole covers are for drinking water.



	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	


MAIN FRONT VIEW OF A 15M X 48M PETROLEUM STORAGE COMMERCIAL DECK BARGE. SHOWING THE HEADLONG




  6.75c.m                       1.50c.m                        6.75c.m


                              15m

UPPER FENDER.
                                                    BRAZE BRACKET
             BOTTOM FENDER.
                            EASY CONNECTING POINT TO A TUGBOAT.
